

**BẢNG BÁO GIÁ Aver EVC170**

*Ngày 17/12/2022*

***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **Aver EVC170** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |  |
| --- | --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** | |
| 1 | Package contentsMain system unit (codec)eCam PTZ IV cameraEVC microphone arrayIR remote control with batteriesPower supplyCablesWarranty cardQuick guideCommunicationsH.323, SIP standards, SIP TLSWebRTC (License Required)Call-Quality bandwidth 64Kbps ~ 8MbpsRJ45 network LAN (10/100/1000)Manual max. bandwidth settingsCameraeCam PTZ IV camera2-megapixel CMOS sensor18X total zoom (12X optical + 1.5X digital)130 pan; +90/-25 tilt72 FOV (H); 43 FOV (V); 82 FOV (diagonal)People video resolutionsHD 1080p (1920 x 1080), up to 60fpsHD 720p (1280 x 720)480p (848 x 480)4CIF (704 x 576)CIF (352 x 288)SIF (352 x 240)All resolutions at 30fpsContent video resolutionsHDMI-supported resolutionsOutput resolutions:1080p (1920 x 1080)720p (1280 x 720)D1 (720 x 480)SXGA (1280 x 1024)XGA (1024 x 768)SVGA (800 x 600)VGA (640 x 480)Up to HD1080p (1920 x 1080) up to 60fpsVideo standardsH.264, H.264 HP, H.264 SVC, H.263+, H.263H.239 dual-video streamsBFCP content sharingVideo features3D denoiseVideo inputsMain camera eCam PTZ IVHDMI/VGA for presentationVideo outputsHDMI x 2VGAAudio standardsG.711, G.722, G.722.1, G.728, G.722.1C, AAC-LD, G729Audio featuresAutomatic gain control (AGC)Advanced noise reduction (NR)Acoustic echo cancellation (AEC)Audio inputsEVC microphone daisy chain up to 4HDMILine-in (3.5 mm)Audio outputsHDMI x 2Line-out (3.5 mm)Other supported standardsH.224, H.225, H.245, H.281, H.323 Annex Q, H.460RTP, RTCP, H.350, SRTP, H.235, HTTP, HTTPs, Telnet, DHCP, DNSUser interfaceSingle/dual-monitor layout stylesUser-friendly OSD (23 supported languages: English, Traditional Chinese, Simplified Chinese, Czech, Danish, Dutch, Finnish, French, German, Hungarian, Italian, Japanese, Korean, Norwegian, Polish, Portuguese, Brazil, Romanian, Russian, Spanish, Swedish, Thai, Turkish, Vietnamese)Display/edit site nameNetwork10/100/1000MbpsNAT/firewall traversal (H.460)High Efficiency Lost Packet Recovery (HELPeR)API support via TelnetPacket Loss Recovery (PLR)Wake-on-LAN (WOL) supportIPv4 and IPv6 supportNetwork testQuality of service (QoS)VLAN (802.1Q / 802.1P)EAP 802.1xSecurityAES (Advanced Encryption Standard) function (128-bit) and H.235Password protection for system settingsPassword protection for remote system managementWeb management toolRemote managementLive monitoringFirmware updatePhonebook download/upload/editRestore system settingsExport call historyHTTP and HTTPsValue-added featuresMeeting recording In-meeting and offline recordingSave directly to USB flash driveSupports screen re-layout during playbackPlayback and file conversion via VCPlayer software (.MOV and .MP4 format)EZMeetup / EZMeetup Plus software/App 30-day for free trialConnect with H.264 and H.264 HP video codecsReceive resolution up to full HD 1080p at 30fpsTransmit resolution up to full HD 1080p at 30fpsSupport content sharing, capturing and recordingEZDraw App Import .JPG, .PNG, .GIF and .BMP filesExport .PNG filesConnect up to 10 devicesScreenShare software (Wirelessly share content)VCLink software (control and sharing in smartphone)Dual-monitor support output (video and content sharing)Speed dialing via hot keys (10 sets)Camera presets (100 positions)Firmware updates via USB flash driveScreensaver and auto power-off modeNetwork Time Protocol (NTP)SnapShotSupports SIP voice callsiSCSI storage device settingsBuilt-in meeting serverSupports AVer Register Server (ARS)Far-end Camera ControlMeeting ID methodPower supplyAC 100V ~240V, 50/60 HzConsumption: EIAJ 12V, 5AEnvironmental dataOperation temperature: 0 ~ 40COperation humidity: 20 ~ 80%Storage temperature: -20 ~ 60CStorage humidity: 20 ~ 80%Physical characteristicsPackage dimensions: 376 x 300 x 243 mmPackage weight: 6.99kg (14.31lbs)Main system (codec): 320 x 262.7 x 37.2 mmeCam PTZ IV: 180 x 144 x 184 mmEVC microphone array: 131.9 x 118.6 x 25.5 mmOptional accessoriesAdditional microphoneCamera mountUSB-to-RS232 converterSoftware optionsWebRTC LicenseWarranty\*\*Camera/Codec/Microphone: 3+2 yearAccessories: 1 year\*G.722.1/G.722.1C, licensed from Polycom \*\*Please register online to receive a free, 2 year warranty extension. For detailed warranty information, please contact an AVer representative. | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* | |
| **Giá tiền** | 0 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 0 |
|  | |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | | | 0 |

|  |
| --- |
| **Điều kiện thương mại:**  \* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá \* Miễn phí giao hàng trong nội thành Hà Nội \* Thời gian giao hàng: Thỏa thuận \* Bảo hành tại: Theo đúng tiêu chuẩn của hãng \* Thanh toán : Tiền mặt hoặc chuyển khoản  \* Thông tin tài khoản:   *Công ty Cổ phần Công Nghệ Phúc An  Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN  TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|