

**BẢNG BÁO GIÁ Camera hội nghị tuyền hình Aver PTZ310**

*Ngày 19/12/2022*

 ***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **Camera hội nghị tuyền hình Aver PTZ310** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |
| --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** |
| 1 | Đặc tnh kỹ thuậtCameraImage sensor1/2.8 1080p 60fps Exmor CMOSEffective picture elementsApprox. 2.1 MegapixelsOutput ResolutionAuto1080P@60, 1080P@59.94, 1080P@50, 1080i@60, 1080i@59.94, 1080i@50, 1080P@30, 1080P@29.97, 1080P@25, 720P@60, 720P@59.94, 720P@50Minimum Illumination0.4 lux (IRE50, F1.6, 30FPS)S/N ratio 50dBGainAuto/ManualTV Line800 (center/wide), 700 (corner/wide)Shutter Speed1/1 s to 1/32,000 sExposure ControlAuto, Manual, Priority AE( Shutter, IRIS), BLCWhite balanceAuto/Indoor/Outdoor/One-push/Manual( 2500 - 10000)Optical Zoom12XDigital Zoom12XHorizontal Viewing Angle72.5 (Wide) ~ 6.3 (Tele)Focal lengthf = 3.9 mm (Wide) ~ 46.8 mm (Tele)Aperture (Iris)F = 1.6 (Wide) ~ 2.8 (Tele)Minimum working distance0.3 m (Wide), 1.5 m (Tele)Pan/Tilt AnglePan: -+ 130, Tilt: +90/-30Pan/Tilt Speed (manual)Pan: 0.1~100/sec, Tilt: 0.1~100/secPreset SpeedPan: 200/sec, Tilt: 200/secPreset Position10 (IR), 255 (RS232)Camera Control - IRYesCamera Control - InterfaceRS232 (DIN8) / RS422 (RJ45)Camera Control - ProtocolVISCA (RS-232/RS422/IP), CGI (IP)Image ProcessingNoise Reduction (2/3D), Filp, MirrorPower FrequencyAuto/50Hz/60Hzm thanhAudio - Channel2ch (stereo)Audio - CodecAAC-LC (48/44.1/32/24K), G.711/PCM (16K/8K)Audio - Sample Rate48/44.1/32/24/16/8KhzGiao diệnVideo Output3G-SDI, HDMI, IPAudio Output3G-SDI, HDMI, IPAudio InputMIC/Line inTổng quanPower RequirementAC100V-AC240V to DC12V/5APoEPOE+ (IEEE 802.3at), Class 4Operating ConditionTemperature: 0C ~ +40C; Humidity: 20% ~80%Storage ConditionTemperature: -20C ~ +60C; Humidity: 20% ~ 95%DimensionsL=180 mm，W= 145 mm，H= 183.5 mmWeight1.741 kgApplicationIndoorSecurityKensington slotRemote ControlInfraredAccessoryRemote control, 12V/5A power adapterPht trực tuyếnResolution1920x1080, 1280x720, 960x540, 640x480Network Video Compress FormatH.264 (High Profile), MJPEGMaximum Frame RateH.264: 60fps (1920x1080), MJPEG: 30fps (1920x1080)Bit-rate Control ModeVBR/CBR (selectable)Range of Bit-rate setting512Kbps ~ 32MbpsNetwork Interface10/100/1000Base-TMulti-stream Capability2Network ProtocolIPv4, TCP, UDP, ARP, IMCP, IGMP, HTTP, DHCP, RTP/RTCP, RTSP, VISCA over IPGiao diện người dng trn WebLive Video PreviewYesCamera PTZ ControlPan / Tilt / Zoom / Focus / Preset ControlCamera / Image AdjustmentExposure / White Balance / PictureNetwork ConfigurationDHCP / IP Addr / Gateway / Netmask / DNSPhần mềm hỗ trợDevice IP Searching, Configuration toolWindows Application | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* |
| **Giá tiền** | 0 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 0 |
|  |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | 0 |

|  |
| --- |
| **Điều kiện thương mại:**\* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá\* Miễn phí giao hàng trong nội thành Hà Nội\* Thời gian giao hàng: Thỏa thuận\* Bảo hành tại: Theo đúng tiêu chuẩn của hãng\* Thanh toán : Tiền mặt hoặc chuyển khoản\* Thông tin tài khoản:  *Công ty Cổ phần Công Nghệ Phúc An Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|