

**BẢNG BÁO GIÁ Polycom CX7000 Unified Conference Station for Microsoft Lync**

*Ngày 16/12/2022*

***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **Polycom CX7000 Unified Conference Station for Microsoft Lync** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |  |
| --- | --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** | |
| 1 | Package Includes All systems include: System unit, keyboardand mouse, cables and power supply withlocal cordset CX7000 View system includes:- Polycom EagleEye View camerawith built-in microphones CX7000 HD system includes:- EagleEye III camera and PolycomHDX Microphone ArrayInfrastructure Requirements Microsoft Lync Server 2010 Microsoft Exchange Server 2007, or later,for scheduled meetingsVideo Standards and Protocols RT Video Up to 720p/30fps, for Lync point-topointcalls Up to VGA/30fps, for Lync AVMCU(multipoint or shared content) callsVideo Input 1 x EagleEye HDCI camera input 1 x HDMI 3.1 (for future use; disabledat present) 1 x VGA Content InVideo Out 1 HDMI video out 1 x DVI-I HD video outOutput Resolution for Monitors 1920 x 1200 1920 x 1080 1680 x 1050 1280 x 1024 1280 x 720Content In Video Resolution Resolutions supported:- 1280 x 768- 1280 x 1024 (SXGA)- 1024 x 768 (XGA)- 800 x 600 (SVGA) Content Frame Rate: 5 30 fpsCamera Polycom EagleEye III camera- 1920 x 1080 CMOS imager- 12X optical zoom- Auto focus- 72 FOV Polycom EagleEye View camera- 1920 x 1080 CMOS imager- 4X digital zoom- Manual focus- 55 FOVAudio Input 1 Clink2 for HDX microphone array 1 x 3.5mm stereo mini (PC Audio)Audio Output Audio supported on HDMI output 1 x 3.5mm stereo mini line outAudio Codec Support 7 kHz bandwidth RTAudio 3.4 kHz bandwidth with G.711Audio Enhancement Acoustic Echo Cancellation Automatic gain control Noise suppressionNetwork Connectivity 10/100/1000 Ethernet (RJ45) 2 x USB 3.0 ports 5 x USB 2.0 ports- 2 ports always powered when system isconnected to powerUser Interface Lync client interface- Click-to-join Online Meetings- Receive Lync call (IM, Voice, Video)- Initiate Lync call (IM, Voice, Video)- Share uploaded content- View or actively collaborate on anycontent shared by other participants- Push VGA content- Directory search System configuration Remote administrator accessInput/Output/Control Compact Wireless Keyboard- Localized versions- Integrated camera control forpan-tilt-zoom Wireless mouse with scroll wheelSecurity Partition write protection White list permissions File system lock down Secure password authenticationElectrical Universal auto sensing power supply- Input 100 240 VAC, 50 60 Hz- Output 19 VDC, 7.89A Typical operating voltage/power- 43VA @ 120V / 60 Hz @ .96 PF- 53VA @ 240V / 50 Hz @ .74 PFEnvironmental Specification Operating temperature: 0 40C Operating humidity: 10 80% Non-operating temperature: -40 70C Non-operating humidity (non-condensing):1090% Maximum altitude: 10,000 feetPhysical Characteristics CX7000 system with removable stand- 13.9 x 5.1 x 11 (H/W/D standing)Warranty One-year return to factory parts and labor | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* | |
| **Giá tiền** | 0 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 0 |
|  | |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | | | 0 |

|  |
| --- |
| **Điều kiện thương mại:**  \* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá \* Miễn phí giao hàng trong nội thành Hà Nội \* Thời gian giao hàng: Thỏa thuận \* Bảo hành tại: Theo đúng tiêu chuẩn của hãng \* Thanh toán : Tiền mặt hoặc chuyển khoản  \* Thông tin tài khoản:   *Công ty Cổ phần Công Nghệ Phúc An  Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN  TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|