

**BẢNG BÁO GIÁ Aver CAM520 Pro2 (NEW 2022)**

*Ngày 17/12/2022*

 ***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **Aver CAM520 Pro2 (NEW 2022)** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |
| --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** |
| 1 | CameraSony super-low-light 2M pixel sensor, clear and natural imaging in low-light conditionsResolution: (16:9) 1920 x 1080, 1600 x 900, 1280 x 720, 960 x 540, 848 x 480, 800 x 448, 640 x 360, 424 x 240, 320 x 180; (4:3) 800 x 600, 640 x 480, 480 x 360, 320 x 240 at 60, 30, 15fpsSmartFrame for automatic FOV adjustment to fit all participantsInnovative Preset Framing: Follow presenter based on preset areasTrue WDR up to 120db: Superb backlight compensation technology for optimizing light balance in high-contrast conditionsZoom: 24X total zoom (12X optical zoom)Field of view(D/H/V):84.5/76/48Lens focal length: 3.9 mm (wide) ~ 47.3 mm (tele)Lens F#: 1.8 (wide) ~ 2.8 (tele)Mirror, flip, AE, white balance: auto/manual override via PTZApp2Minimum focus distance: 1.5 mStandard tripod screw holes and Kensington slotPeople-counting API: enterprises and third-party software providers can obtain people-counting data for better understanding of meeting-space usageMotorized Pan Tilt MovementPan: 170Tilt: +90 (up) -30 (down)10 camera presets (via remote control)Fast and quiet pan/tilt movementVideo FormatYUV, YUY2, MJPEG, NV12Network video compression format: H.264Network protocol: RTSP, RTMPConnectivity12V/2A power adaptorMini DIN9 for RS232 in out connection (VISCA control panel and camera daisy chain)USB 3.1 type-B connectorIP (RJ45)USB3.1 Gen1 Type B, backward compatible with USB 2.0UVC (USB video class) 1.1ControlIR remote controlVISCA/pelco P/pelco D via RS232 (128 preset points via VISCA command)Remote side: VISCA over IP, IP (RJ45)UVC/UAC plug and playWebUI: Browser IP access via Chrome (Does not support Internet Explorer)PTZApp 2Package ContentsCAM520 Pro2 unitRemote control5m, USB2.0 type-B to type-A cablePower adapter (10 ft/3 m)QR code cardWall-mount bracket tripod screwMini DIN9 to mini DIN8 RS232 adapterOptional AccessoriesMini DIN8 to D-SUB9 RS232 adapterFoldable TV mountCeiling mountUSB3.1 fiber extender 10m/20m/30mUSB3.1, 3m type-B to type-A cableMountCamera wall-mount bracket includedOptional foldable TV mountOptional ceiling mountSystem RequirementsWindows 7/10Windows 10 Enterprise (IoT) LTSC (version 1809)Mac OS X 10.7 or higherGoogle Chromebook version 29.0.1547.70Hardware Specs\*3.2 GHz Intel Core i5-4460 processor4 GB RAM or moreUSB 3.1 port , backward compatible with USB2.0 portWeb page browser requirementChrome: version 76.x or aboveFirefox: version 69 or aboveIE: Not supportPower SupplyAC 100V ~ 240V, 50/60 HzConsumption: 12V, 2APoE+: 802.3atFree Applications for Meeting Collaboration (Windows and MAC)EZManager 2 : Camera Central Management softwarePTZApp 2EZLive\*Only available in Windows PC. Doesn't support in MAC PC.Remotely manage group FW/SW updates, camera control, and settingsSupport Virtual Streaming function.\*Compatible with Skype for business far-end controlUpgrade firmware automatically or manuallyControl cameraSet parameters and adjust camera imageDiagnose operating statusView live videoReal-time streaming / annotating / image capturing / video recordingEnvironmental DataOperation temperature: 0C ~ 40COperation humidity: 20% ~ 80%Storage temperature: -20C ~ 60CStorage humidity: 20% ~ 80%DimensionsPackage dimensions: 256 x 256 x 274 mmPackage weight: 3.335 kg/7.35 lbsCamera: 182 x 142.7 x 153 mm/1.47 kgRemote control: 200 x 50 x 21 mm/0.09 kgWarrantyCamera: 3 yearsAccessories: 1 yearCompatible Applications\*\* Specifications may vary depending on countries and are subject to change without notice.Zoom, Microsoft Teams, Skype for Business, Skype, Google Meet, Intel Unite, RingCentral, BlueJeans, V-Cube, LiveOn, CyberLink U Meeting, TrueConf, Adobe Connect, Cisco Webex, Fuze, GoToMeeting, Vidyo, vMix, WebRTC, Wirecast, XSplit\* Specifications may vary depending on countries and are subject to change without notice. | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* |
| **Giá tiền** | 45,000,000 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 45,000,000 |
|  |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | 45,000,000 |

|  |
| --- |
| **Điều kiện thương mại:**\* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá\* Miễn phí giao hàng trong nội thành Hà Nội\* Thời gian giao hàng: Thỏa thuận\* Bảo hành tại: Theo đúng tiêu chuẩn của hãng\* Thanh toán : Tiền mặt hoặc chuyển khoản\* Thông tin tài khoản:  *Công ty Cổ phần Công Nghệ Phúc An Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|