

**BẢNG BÁO GIÁ Aver CAM520**

*Ngày 17/12/2022*

 ***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **Aver CAM520** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |
| --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** |
| 1 | Package contentsCameraRemote control5m Micro USB 2.0 Type-B to Type-A cablePower supplyQuick-start guideTabletop/wall/ceiling mount6.35mm tripod mounting screwVelcroCameraFull HD 1080p 60fpsPan: 130; 0.45 stepTilt: +90/-25; 0.25 stepField of view (H): 72.5 (wide) ~ 6.3 (tele)Sensor: 1/2.8 low lux CMOS 2M pixelResolution: full HD 1080p (1920x1080), HD 720p (1280x720), PAL (1024x576), VGA (640x480), QVGA (320x240), QQVGA (160x120) at 60fps, 30fps and 15fpsScan: progressiveZoom: 18X total zoom (12X optical zoom)Lens focal length: 3.9mm (wide) ~ 47.3mm (tele)Lens F#: 1.8 (wide) ~ 2.8 (tele)Auto IrisS/N ratio: 50dBMinimum illumination: 1 lx (50 IRE, F1.6, shutter 1/30)2D and 3D denoiseBacklight compensationFlip, mirrorMinimum working distance: 1.5 meterInclude table/wall/ceiling mountKensington slotRemote controlIR (Infrared)10 camera presets (100 presets via VISCA)System requirements\*Windows 7/ 8/8.1/10Mac OS X 10.7 or higherGoogle Chromebook version 29.0.1547.70, Platform 4319.79.0Hardware requirements\*2.4 GHz Intel Core 2 Duo processor2 GB RAM or moreUSB 2.0 portPower supplyAC 100V ~ 240VConsumption: EIAJ 12, 4AEnvironmental dataPhysical characteristics: 0~40COperation humidity: 20%~80%Storage temperature: -20~60CStorage humidity: 20%~80%Physical characteristicsPackage dimensions: 370 x 252 x 275mmPackage weight: 4.16kg/9.17lbsCamera: 180 x 140 x 182mm/1.5kgRemote control: 200 x 50 x 20mm/0.091kgOptional accessoriesRS232 adapterCompliance and toolsYUV, MJPEG, H.264 SVC, AVC (high and base profile)Multi-stream capableUSB 2.0UVC (USB Video Class) 1.1 with H.264 extensionVISCA via RS232\*Downloadable diagnostic tool, field firmware upgrade tool, App for advanced features and settings\*Please check AVer product web page for compatible VISCA commands and devices.PTZAppFree download on Windows and Mac computersCompatible with SkypeTM Plugin for answering and hanging up via remote controlUpgrade firmware automatically or manually control cameraSet parameters and adjust camera imageDiagnose operating statusView live videoWarranty\*\*3-year: camera1-year: accessoriesCompatible applicationsSkype, Skype for Business, V-CUBE, Google Hangouts, FaceTime, Cisco Webex, GoToMeeting, Adobe Connect, BlueJeans, Zoom, Vidyo, Fuze, WebRTC, CyberLink U Meeting\* For Full HD support, please check with your software application provider for system/hardware requirements.
\*\* Please register online to receive free 2 year warranty extension. For detailed warranty information, please contact an AVer local representative.
\*\*\* Specifications may vary depending on countries and are subject to change without notice. | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* |
| **Giá tiền** | 30,000,000 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 30,000,000 |
|  |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | 30,000,000 |

|  |
| --- |
| **Điều kiện thương mại:**\* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá\* Miễn phí giao hàng trong nội thành Hà Nội\* Thời gian giao hàng: Thỏa thuận\* Bảo hành tại: Theo đúng tiêu chuẩn của hãng\* Thanh toán : Tiền mặt hoặc chuyển khoản\* Thông tin tài khoản:  *Công ty Cổ phần Công Nghệ Phúc An Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|