

**BẢNG BÁO GIÁ Aver VB342+**

*Ngày 17/12/2022*

 ***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **Aver VB342+** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |
| --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** |
| 1 | - Camera + Sony Exmore sensor: Ultra crystal-clear image support up to 4K + Frame rate: 4K 30fps; 1080p, 720p, 960 x 540, 848 x 480, 800 x 448, 640 x 480, 640 x 360, 424 x 240, 320 x 240, 320 x 180 at 60, 30, 15fps + SmartFrame SmartSpeaker: Automatic FOV adjustment to fit all participants and focus on the speaker + 120 wide field of view + True WDR up to 120 db: Superb back light compensation technology for optimizing light balance in high-contrast conditions + Digital zoom rate up to 4X leveraging 4K sensor + 3D denoise technology maintains clear and natural imaging in low light conditions + Mirror, AE, white balance: Auto, manual override via PTZApp + Minimum focus distance: 80 cm + Analytics API: Enterprises and third-party software providers can obtain people-counting data for better understanding of meeting-space usage- Motorized Pan and Tilt Movement + Pan: Total horizontal viewing area 180 + Tilt: Total vertical viewing area 105 + 10 camera presets (through remote control) + Fast and quiet pan tilt movement- Audio + Microphones: 2 unidirectional microphones supporting 6 m pickup + 5Wx2 stereo full range speakers with professional bass port tuned for communication + Volume up to 96 dB SPL at 1/2 meter +Echo cancellation + Noise suppression + 3.5 mm Line-in (aux) cable connects BYOD smartphones or PCs as speakerphones- HDMI + DisplayLink: Built-in USB 3.1 (Gen 1) to HDMI adapter + 1080p HDMI output to TV\*\*\*\* Win7/8 OS: Must install DisplayLink driver via AVer PTZApp- Connectivity + 12V/5A power adaptor + Mini DIN6 for RS232 connection + USB type C connector + HDMI out connection (DisplayLink) + Phone in (3.5 mm audio jack) + Mic input + Wireless connection with mobile devices\*\*\*\*Wireless function is not supported in the USA and some other countries. Please contact a local agent for details.
\*\*Wireless connection does not support wireless speakerphone devices.- Video Format + YUV, YUY2, M-JPEG- USB + 3.1 Gen 1, backward compatible USB 2.0 + UVC (USB Video Class) 1.1- Control + IR remote control + VISCA/pelco P/pelco D via RS232 + UVC/UVA plug-and-play + PTZApp- Security and Mount + Camera wall-mount bracket included | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* |
| **Giá tiền** | 0 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 0 |
|  |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | 0 |

|  |
| --- |
| **Điều kiện thương mại:**\* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá\* Miễn phí giao hàng trong nội thành Hà Nội\* Thời gian giao hàng: Thỏa thuận\* Bảo hành tại: Theo đúng tiêu chuẩn của hãng\* Thanh toán : Tiền mặt hoặc chuyển khoản\* Thông tin tài khoản:  *Công ty Cổ phần Công Nghệ Phúc An Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|