

**BẢNG BÁO GIÁ Aver VC520 Pro2**

*Ngày 17/12/2022*

***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **Aver VC520 Pro2** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |  |
| --- | --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** | |
| 1 | CameraSony super-low-light 2M pixel sensor for clear and natural imaging in low-light conditionsResolution: (16:9) 1920 x 1080, 1600 x 900, 1280 x 720, 960 x 540, 848 x 480, 800 x 448, 640 x 360, 424 x 240, 320 x 180; (4:3) 800 x 600, 640 x 480, 480 x 360, 320 x 240 at 60, 30, 15fpsSmartFrame for automatic FOV adjustment to fit all participantsInnovative Preset Framing: Follow presenter based on preset areasTrue WDR up to 120dB: Superb backlight compensation technology for optimizing light balance in high-contrast conditionsZoom: 18X total zoom (12X optical zoom)Field of view(D/H/V): 84.5/76/48Lens focal length: 3.9 mm (wide) ~ 47.3 mm (tele)Lens F#: 1.8 (wide) ~ 2.8 (tele)Mirror, Flip, AE, white balance: auto, manual override via PTZApp 2Minimum focus distance: 1.5 mStandard tripod screw holes and Kensington slotPeople-counting API: enterprises and third-party software providers can obtain people-counting data for better understanding of meeting-space usageMotorized Pan Tilt MovementPan: 170Tilt: +90 (up) -30 (down)10 camera presets (via remote control)Fast and quiet pan tilt movementVideo FormatYUV, YUY2, MJPEG, NV12Network video compression format: H.264Network protocols: RTSP, RTMPSpeakerphoneFull duplex microphone array with echo cancellationAdvanced noise suppressionDual-microphone array3.5 mm phone-in jack3.5 mm line outSpeaker: 6W, Adjustable to 90dB SPL at 0.5 mTouch controls for volume down/up, mute, phone input, call, and hang-upBridge phone-in and USB into one callSecurity: Kensington slotAudio FormatAAC-LCNetwork protocol: RTSP, RTMPConnectivity12V/5A power adaptorMini DIN9 for RS232 in out connection (VISCA control panel and camera daisy-chain)USB 3.1 Type-B connectorIP (RJ45)Environmental DataOperation temperature: 0C ~ 40COperation humidity: 20% ~ 80%Storage temperature: -20C ~ 60CStorage humidity: 20% ~ 80%DimensionsPackage dimensions: 259 x 259 x 349 mmPackage weight: 5.4 kgCamera: 142.7 x 153 x 182 mm/1.45 kgSpeakerphone: 220 x 181.5 x 49.5 mm/0.85 kgRemote control: 200 x 50 x 21 mm/0.09 kgPackage ContentsVC520 Pro2 CameraVC520 Pro2 SpeakerphoneRemote controlPower adapterPower cord (6 ft/1.8 m)USB2.0 type-B to type-A cable (16.5 ft/5 m)Camera to Speakerphone Cable (33ft/ 10m)3.5 mm aux cable (3 ft/0.9 m)QR code cardWall-mount bracket tripod screwUSB3.1 Gen 1 Type-B, backward compatible with USB 2.0UVC (USB video class) 1.1UAC (USB audio class) 1.0ControlIR remote controlVISCA/Pelco-P/Pelco-D via RS232 (128 preset points via VISCA command)Remote side: VISCA over IP, IP (RJ45)UVC/UAC plug-and-playWebUI: Browser IP access via Chrome (does not support Internet Explorer)PTZApp 2MountCamera wall-mount bracket includedOptional foldable TV mountOptional ceiling mountSystem RequirementsWindows 7/10Mac OS X 10.7 or higherGoogle Chromebook version 29.0.1547.70 or laterWindows 10 Enterprise (IoT) LTSC (version 1809)Hardware Specs3.2 GHz Intel Core i5-4460 Processor or higher4 GB RAM or moreUSB 3.1 port, backward compatible with USB 2.0 portWeb page browser requirementChrome: version 76.x or aboveFirefox: version 69 or aboveIE: Not supportPower SupplyAC 100V ~ 240V, 50/60 HzConsumption: 12V, 5AFree Applications for Meeting Collaboration (Windows and Mac)EZManager 2: Camera Central Management softwarePTZApp 2EZLiveRemotely group FW/SW upgrades, control the camera, and configure settingsUpgrade firmware automatically or manuallyControl cameraSet parameters and adjust camera imageDiagnose operating statusView live videoReal-time streaming / annotating / snapshots / video recordingOptional AccessoriesMini DIN8 to D-SUB9 RS232 adapterExpansion SpeakerphoneExpansion MicrophoneFoldable TV mountUSB3.1 fiber extender 10m/20m/30mUSB3.1 type-B to type-A cable 3mCeiling mountWarrantyCamera / Speakerphone: 3 yearsAccessories: 1 yearCompatible Applications\*\*Specifications may vary depending on countries and are subject to change without notice.Zoom, Microsoft Teams, Skype for Business, Skype, Google Meet, Intel Unite, RingCentral, BlueJeans, V-Cube, LiveOn, CyberLink U Meeting, TrueConf, Vidyo, Adobe Connect, Cisco Webex, Fuze, GoToMeeting, Microsoft Lync, vMix, WebRTC, Wirecast, XSplit\* Specifications may vary depending on countries and are subject to change without notice. | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* | |
| **Giá tiền** | 0 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 0 |
|  | |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | | | 0 |

|  |
| --- |
| **Điều kiện thương mại:**  \* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá \* Miễn phí giao hàng trong nội thành Hà Nội \* Thời gian giao hàng: Thỏa thuận \* Bảo hành tại: Theo đúng tiêu chuẩn của hãng \* Thanh toán : Tiền mặt hoặc chuyển khoản  \* Thông tin tài khoản:   *Công ty Cổ phần Công Nghệ Phúc An  Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN  TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|