

**BẢNG BÁO GIÁ THIẾT BỊ HỘI NGHỊ TRUYỀN HÌNH YEALINK VC200-WP**

*Ngày 10/01/2023*

 ***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **THIẾT BỊ HỘI NGHỊ TRUYỀN HÌNH YEALINK VC200-WP** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |
| --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** |
| 1 | Package includes:
 VC200 Codec
(integrate codec/camera/microphone/bracket)
 VCR11 Remote Control
 PoE Adapter
 WPP20 Wireless Presentation Pod (optional)
 VCH50 Video Conferencing Hub (optional)
Ultra HD 4K Camera
 Ultra HD 4K camera
 1920 x 1080 video resolution
 30 frame rate
 4x e-PTZ camera
 Horizontal field of view: 103
 Beauty shot
Microphone
 Built-in six beamforming microphone arrays
 16ft / 5 meters voice pickup distance
 Wireless microphone (optional)
 Conference phone CP960 (optional)
Video Standard and Network Suitability
 Video codecs:
H.265/HEVC, H.264 High Profile, H.264, H.263
 Forward Error Correction (FEC)
 Anti 30% video packet loss
 Bandwidth dynamic adaptive adjustment
 Shared content and audio preference strategy
 Bandwidth/protocol/audiovideo call auto adaptive
Audio Features
 Audio codecs:
- Opus, 8~48kHz sampling rate
- 14kHz bandwidth with G.722.1C
- 7kHz bandwidth with G.722.1
- 3.4kHz bandwidth with G.711 (PCMA/PCMU)
 Audio technology:
- Acoustic echo cancellation
- Automatic gain control
- Yealink Noise Proof Technology
- CNG, PLC, AJB, De-Rerb
Operating System
 Based on Android 7.1
Call Features
 1080P30 people + 1080P30 content sharing
video quality
 Video Layout: Picture-in-picture (PIP)
 Video/audio recording and playback
 Screenshots in USB flash drive or local storage
 Group dial
 YMS meeting control:
- invite/remove
- mute/unmute participates
- lock
 DND (do not disturb), call statistics
 Auto answer, mute, call waiting
 Virtual keyboard
 Local directory: 500 entries
 Call history: all/missed/received/dialed
 LDAP phonebook
 Multi-language support
 Additional five-way audio call
Standard Communication Protocol
 H.323/SIP
 Dual stream protocol: H.239 (H.323)/BFCP (SIP)
 FECC: H.224/H.281, Sony VISCA and PELCO D/P
 H.323 protocol suite: H.245, H.225, H.235, H.241
 Gatekeeper account and SIP account
Network and Security Features
 Built-in dual-band Wi-Fi (2.4GHz/5GHz):
- connect to a Wi-Fi network
- serve as a Wi-Fi hotspot
 Built-in Bluetooth
 IPv4 and IPv6, DHCP/static IP
 HTTP/HTTPS web server
 RS232/HTTP API for control system integration
 SRTP/TLS, AES 128-bit encryption
 QoS: 802.1p/q, Diff-serv
 VLAN, IEEE802.1X, LLDP-MED
 Anti-attack
 Network diagnosis: Ping, trace route
 Time and date synchronization using SNTP
 Built-in certificate
NAT and Firewall Traversal
 ICE/TURN/STUN
 H.460
 NAT (manual/auto mode)
 Yealink intelligent firewall traversal | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* |
| **Giá tiền** | 0 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 0 |
|  |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | 0 |

|  |
| --- |
| **Điều kiện thương mại:**\* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá\* Miễn phí giao hàng trong nội thành Hà Nội\* Thời gian giao hàng: Thỏa thuận\* Bảo hành tại: Theo đúng tiêu chuẩn của hãng\* Thanh toán : Tiền mặt hoặc chuyển khoản\* Thông tin tài khoản:  *Công ty Cổ phần Công Nghệ Phúc An Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|