

**BẢNG BÁO GIÁ THIẾT BỊ HỘI NGHỊ TRUYỀN HÌNH YEALINK VC200-WP**

*Ngày 10/01/2023*

***Kinh gửi***: Quý khách hàng

**Công ty Phúc An** xin trân trọng gửi tới **Quý khách** bảng báo giá **THIẾT BỊ HỘI NGHỊ TRUYỀN HÌNH YEALINK VC200-WP** cùng với thông số sản phẩm cụ thể như sau:

|  |  |  |  |
| --- | --- | --- | --- |
| **STT** | **THÔNG TIN SẢN PHẨM** | **HỈNH ẢNH & ĐƠN GIÁ** | |
| 1 | Package includes: VC200 Codec (integrate codec/camera/microphone/bracket) VCR11 Remote Control PoE Adapter WPP20 Wireless Presentation Pod (optional) VCH50 Video Conferencing Hub (optional) Ultra HD 4K Camera Ultra HD 4K camera 1920 x 1080 video resolution 30 frame rate 4x e-PTZ camera Horizontal field of view: 103 Beauty shot Microphone Built-in six beamforming microphone arrays 16ft / 5 meters voice pickup distance Wireless microphone (optional) Conference phone CP960 (optional) Video Standard and Network Suitability Video codecs: H.265/HEVC, H.264 High Profile, H.264, H.263 Forward Error Correction (FEC) Anti 30% video packet loss Bandwidth dynamic adaptive adjustment Shared content and audio preference strategy Bandwidth/protocol/audiovideo call auto adaptive Audio Features Audio codecs: - Opus, 8~48kHz sampling rate - 14kHz bandwidth with G.722.1C - 7kHz bandwidth with G.722.1 - 3.4kHz bandwidth with G.711 (PCMA/PCMU) Audio technology: - Acoustic echo cancellation - Automatic gain control - Yealink Noise Proof Technology - CNG, PLC, AJB, De-Rerb Operating System Based on Android 7.1 Call Features 1080P30 people + 1080P30 content sharing video quality Video Layout: Picture-in-picture (PIP) Video/audio recording and playback Screenshots in USB flash drive or local storage Group dial YMS meeting control: - invite/remove - mute/unmute participates - lock DND (do not disturb), call statistics Auto answer, mute, call waiting Virtual keyboard Local directory: 500 entries Call history: all/missed/received/dialed LDAP phonebook Multi-language support Additional five-way audio call Standard Communication Protocol H.323/SIP Dual stream protocol: H.239 (H.323)/BFCP (SIP) FECC: H.224/H.281, Sony VISCA and PELCO D/P H.323 protocol suite: H.245, H.225, H.235, H.241 Gatekeeper account and SIP account Network and Security Features Built-in dual-band Wi-Fi (2.4GHz/5GHz): - connect to a Wi-Fi network - serve as a Wi-Fi hotspot Built-in Bluetooth IPv4 and IPv6, DHCP/static IP HTTP/HTTPS web server RS232/HTTP API for control system integration SRTP/TLS, AES 128-bit encryption QoS: 802.1p/q, Diff-serv VLAN, IEEE802.1X, LLDP-MED Anti-attack Network diagnosis: Ping, trace route Time and date synchronization using SNTP Built-in certificate NAT and Firewall Traversal ICE/TURN/STUN H.460 NAT (manual/auto mode) Yealink intelligent firewall traversal | ***Lưu ý:*** *Hình ảnh có thể chưa hoàn toàn chính xác theo thực tế* | |
| **Giá tiền** | 0 |
| **Số lượng** | 1 |
| **Giảm giá** | 0% |
| **Thành tiền** | 0 |
|  | |
| **TỔNG GIÁ TRỊ CHƯA BAO GỒM THUẾ VAT (10%)** | | | 0 |

|  |
| --- |
| **Điều kiện thương mại:**  \* Báo giá có giá trị trong 07 ngày, tính từ ngày trên báo giá \* Miễn phí giao hàng trong nội thành Hà Nội \* Thời gian giao hàng: Thỏa thuận \* Bảo hành tại: Theo đúng tiêu chuẩn của hãng \* Thanh toán : Tiền mặt hoặc chuyển khoản  \* Thông tin tài khoản:   *Công ty Cổ phần Công Nghệ Phúc An  Đ/C: Số 15 Ngõ Ao Dài, Đường Đê Tô Hoàng, Phường Cầu Dền, Quận Hai Bà Trưng, HN  TK số : 088704066783333 tại Ngân hàng TMCP Quốc Tế Việt Nam (VIBank) – Thanh Xuân* |
|
|
|
|
|
|